### uVision2 Project, (C) Keil Software
### Do not modify !

Target (3 XData Areas on T89C51RD2), 0x0000 // Tools: 'MCS-51'

Group (Source Files)
Group (Documentation)

File 1,1,<.\MAIN.C><MAIN.C> 0x0 
File 1,2,<.\XBANKING.A51><XBANKING.A51> 0x0 
File 1,1,<.\Eeprom.c><Eeprom.c> 0x0 
File 2,5,<.\ABSTRACT.TXT><ABSTRACT.TXT> 0x0 


Options 1,0,0  // Target '3 XData Areas on T89C51RD2'
 Device (AT89C51ED2)
 Vendor (Atmel)
 Cpu (IRAM(0-0xFF) IROM(0-0xFFFF) XRAM (0-0x6FF) CLOCK(33000000) MODP2)
 FlashUt ("batchisp" (-device $D -hardware RS232 -port COM1 -baudrate 19200 -operation MEMORY FLASH LOADBUFFER %H PROGRAM))
 StupF ("LIB\STARTUP.A51" ("Standard 8051 Startup Code"))
 FlashDR ()
 DevID ()
 Rgf (at89c51xd2.h)
 Mem ()
 C ()
 A ()
 RL ()
 OH ()
 DBC_IFX ()
 DBC_CMS ()
 DBC_AMS ()
 DBC_LMS ()
 UseEnv=0
 EnvBin ()
 EnvInc ()
 EnvLib ()
 EnvReg (˙Atmel\)
 OrgReg (˙Atmel\)
 TgStat=16
 OutDir (.\)
 OutName (XData3)
 GenApp=1
 GenLib=0
 GenHex=0
 Debug=1
 Browse=1
 LstDir (.\)
 HexSel=0
 MG32K=0
 TGMORE=0
 RunUsr 0 0 <>
 RunUsr 1 0 <>
 BrunUsr 0 0 <>
 BrunUsr 1 0 <>
 SVCSID <>
 MODEL5=0
 RTOS5=0
 ROMSZ5=2
 DHOLD5=0
 XHOLD5=0
 T51FL=2212464
 XT51FL=0
 CBANKS5=0
 XBANKS5=0
 RCB51 { 0,0,0,0,0,255,255,0,0 }
 RXB51 { 0,0,0,0,0,0,0,0,0 }
 OCM51 { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 OCR51 { 0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 IRO51 { 1,0,0,0,0,0,0,1,0 }
 IRA51 { 0,0,0,0,0,0,1,0,0 }
 XRA51 { 0,0,0,0,0,0,7,0,0 }
 XRA512 { 0,0,0,0,0,0,0,0,0 }
 IROM512 { 0,0,0,0,0,0,0,0,0 }
 C51FL=21630224
 C51VA=0
 C51MSC ()
 C51DEF ()
 C51UDF ()
 INCC5 ()
 AX51FL=4
 AX51MSC (LINES)
 AX51SET ()
 AX51RST ()
 INCA5 ()
 PropFld { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 IncBld=1
 AlwaysBuild=0
 GenAsm=0
 AsmAsm=0
 PublicsOnly=0
 StopCode=3
 CustArgs ()
 LibMods ()
 BankNo=65535
 LX51FL=288
 LX51OVL ()
 LX51MSC ()
 LX51DWN ()
 LX51LFI ()
 LX51ASN ()
 LX51RES ()
 LX51CCL ()
 LX51UCL (HDATA_EEPROM  (X:0x020000-X:0x0207FF),\~HDATA   (X:0x010000-X:0x0103FF)\~)
 LX51CSC ()
 LX51UCS ()
 LX51COB ()
 LX51XDB ()
 LX51PDB ()
 LX51BIB ()
 LX51DAB ()
 LX51IDB ()
 LX51PRC ()
 LX51STK ()
 LX51COS ()
 LX51XDS ()
 LX51BIS ()
 LX51DAS ()
 LX51IDS ()
  OPTDL (S8051.DLL)()(DP51.DLL)(-pATED2)(S8051.DLL)()(TP51.DLL)(-pATED2)
  OPTDBG 133117,0,()()()()()()()()()() (BIN\MON51.DLL)()()()
 FLASH1 { 1,0,0,0,0,0,0,0,255,255,255,255,0,0,0,0,0,0,0,0 }
 FLASH2 ()
 FLASH3 ("batchisp" (-device $D -hardware RS232 -port COM1 -baudrate 19200 -operation MEMORY FLASH LOADBUFFER %H PROGRAM))
 FLASH4 ()
EndOpt

