 ***************************************************************************
                        PSDsoft Express Version 8.30
                    Output of PSD Configurations
 ***************************************************************************
  PROJECT    : project                        DATE : 11/30/2004
  DEVICE     : uPSD3334D                      TIME : 21:01:43
 ***************************************************************************


 ==== Bus Interface ==== 

 Data Bus Width                                                    = 8-Bit 
 Address/Data Mode                                                 = Multiplexed 
 ALE/AS Signal                                                     = Active High 
 Control Signals                                                   = /WR,/RD,/PSEN 
 Main PSD flash memory will reside in this space at power-up       = Program/Data space 
 Secondary PSD flash memory will reside in this space at power-up  = Program space 


 ==== Other Configurations ====  

 Enable Chip-Select Input(/CSI)      = OFF 
 Enable Standby Voltage Input (PC2)  = OFF 
 Enable Standby-on Indicator (PC4)   = OFF 
 Enable RDY/Busy function (PC3)      = OFF 
 Load Micro-Cell on edge 
 Security Protection                 = OFF 


 ==== JTAG Configurations ====  

 Enable TMS/TCK/TDI/TDO on PC0/PC1/PC5/PC6, respectively = ON 
 Enables JTAG signal TSTAT on PC3 = OFF 
 Enables JTAG signal TERR on PC4 = OFF 
 User Code = FFFFFFFF

 ==== Flash Sector Protect ====  

 Flash Sector 0 is unprotected 
 Flash Sector 1 is unprotected 
 Flash Sector 2 is unprotected 
 Flash Sector 3 is unprotected 
 Flash Sector 4 is unprotected 
 Flash Sector 5 is unprotected 
 Flash Sector 6 is unprotected 
 Flash Sector 7 is unprotected 
 Flash Boot Sector 0 is unprotected 
 Flash Boot Sector 1 is unprotected 
 Flash Boot Sector 2 is unprotected 
 Flash Boot Sector 3 is unprotected 

