### uVision2 Project, (C) Keil Software
### Do not modify !

Target (89C51RD2 eeprom demo), 0x0000 // Tools: 'MCS-51'

Group (Source Files)
Group (Documentation)

File 1,1,<.\MAIN.C><MAIN.C> 0x0 
File 1,2,<.\XBANKING.A51><XBANKING.A51> 0x0 
File 1,1,<.\eeprom.c><eeprom.c> 0x0 
File 2,5,<.\ABSTRACT.TXT><ABSTRACT.TXT> 0x0 


Options 1,0,0  // Target '89C51RD2 eeprom demo'
 Device (AT89C51RD2)
 Vendor (Atmel)
 Cpu (IRAM(0-0xFF) IROM(0-0xFFFF)  XRAM(0-0x6FF) CLOCK(33000000) MODP2)
 FlashUt ("batchisp" (-device $D -hardware RS232 -port COM1 -baudrate 19200 -operation MEMORY FLASH LOADBUFFER %H PROGRAM))
 StupF ("LIB\STARTUP.A51" ("Standard 8051 Startup Code"))
 FlashDR ()
 DevID ()
 Rgf (at89c51xd2.h)
 Mem ()
 C ()
 A ()
 RL ()
 OH ()
 DBC_IFX ()
 DBC_CMS ()
 DBC_AMS ()
 DBC_LMS ()
 UseEnv=0
 EnvBin ()
 EnvInc ()
 EnvLib ()
 EnvReg (˙Atmel\)
 OrgReg (˙Atmel\)
 TgStat=16
 OutDir (.\)
 OutName (EE2PROM)
 GenApp=1
 GenLib=0
 GenHex=0
 Debug=1
 Browse=1
 LstDir (.\)
 HexSel=0
 MG32K=0
 TGMORE=0
 RunUsr 0 0 <>
 RunUsr 1 0 <>
 BrunUsr 0 0 <>
 BrunUsr 1 0 <>
 SVCSID <>
 MODEL5=0
 RTOS5=0
 ROMSZ5=2
 DHOLD5=0
 XHOLD5=0
 T51FL=2212464
 XT51FL=0
 CBANKS5=0
 XBANKS5=0
 RCB51 { 0,0,0,0,0,255,255,0,0 }
 RXB51 { 0,0,0,0,0,0,0,0,0 }
 OCM51 { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 OCR51 { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 IRO51 { 1,0,0,0,0,0,0,1,0 }
 IRA51 { 0,0,0,0,0,0,1,0,0 }
 XRA51 { 0,0,0,0,0,0,7,0,0 }
 XRA512 { 0,0,0,0,0,0,0,0,0 }
 IROM512 { 0,0,0,0,0,0,0,0,0 }
 C51FL=21630224
 C51VA=0
 C51MSC ()
 C51DEF ()
 C51UDF ()
 INCC5 ()
 AX51FL=4
 AX51MSC (LINES)
 AX51SET ()
 AX51RST ()
 INCA5 ()
 PropFld { 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 IncBld=1
 AlwaysBuild=0
 GenAsm=0
 AsmAsm=0
 PublicsOnly=0
 StopCode=3
 CustArgs ()
 LibMods ()
 BankNo=65535
 LX51FL=292
 LX51OVL ()
 LX51MSC ()
 LX51DWN ()
 LX51LFI ()
 LX51ASN ()
 LX51RES ()
 LX51CCL ()
 LX51UCL (HDATA_EEPROM (X:0x020000-X:0x0207FF))
 LX51CSC ()
 LX51UCS ()
 LX51COB ()
 LX51XDB ()
 LX51PDB ()
 LX51BIB ()
 LX51DAB ()
 LX51IDB ()
 LX51PRC ()
 LX51STK ()
 LX51COS ()
 LX51XDS ()
 LX51BIS ()
 LX51DAS ()
 LX51IDS ()
  OPTDL (S8051.DLL)()(DP51.DLL)(-pATRD2)(S8051.DLL)()(TP51.DLL)(-pATRD2)
  OPTDBG 131581,0,()()()()()()()()()() (BIN\MON51.DLL)()()()
 FLASH1 { 1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0 }
 FLASH2 ()
 FLASH3 ("batchisp" (-device $D -hardware RS232 -port COM1 -baudrate 19200 -operation MEMORY FLASH LOADBUFFER %H PROGRAM))
 FLASH4 ()
EndOpt

